The Run Status of BESII in 1999/2000

Tao Hu IHEP

June 6, 2000

ffl Operation and Data taking ffl Performance of BESII ffl Summary

32

33

34

Table3: Performance of BESII

Sub-system Status VC Normal MDC Field wires ( L4:1, L6:2 ) TOF Normal BSC 2 wires broken ESC Wrong amplifiers were used

¯ Normal

Luminosity Connection of delay Trigger Normal Online High bit set to 1 System crash (error-tolerance,network) Support Normal

ffl After terminators were added to the SC RESET and GATE signal to

reduce their reflection, the MDC hot channels and MDC track finding hot channels were obviously decreased.’

Summary

¨ The J/ψ data taking is successful .

22.5 Million J/ψ events have got !

¨ The performance of BESII is reasonably good

though more aging problem.

¨ Thanks to all BES collaboration and BEPC

people !

36

37

38

39

40

41